Marlon Guanoluisa:

* Change all the wires for both motors and crimping the headers of them to the connection terminal crimps and introduced them into the interface connector.
* Rewired again the connections between the motor drive board to the motors and to the power source for the encoders.
* Assemble and disassemble the buggy because some failures were present and looked for a good spot to place the switch of the battery.
* Help Osama to understand how it is connected the motors and encoders to the motor drive board and discussed the progress of the code for the TD1.